Steps for installation:
1. Run the driver and follow the installation wizard
2. When the wizard is asking for inserting the cable, insert the cable onto the computer
3. Click continue.
4. If the computer is installing the driver automatically from windwos update, please close the automatic installation